**MS500 Optional Engines: (Gasoline / Diesel)**



**QQ图片20161013153901**

|  |  |  |
| --- | --- | --- |
| **Engine Brand** | **Changchai 3M78** | **Kubota D1105** |
| Emission Standard | **Euro Stage V** | **EPA Tier 4 / Euro Stage 5** |
| Cooling system | Water cooling | Water cooling |
| Cylinders | 3 Cylinders | 3 Cylinders |
| Rated Power | 17.65KW (24HP) | 18.5KW (25HP) |
| R.P.M. | 2800r/min | 3000 r/min |

**MS500 Specifications**

|  |  |
| --- | --- |
| ****Model**** | ****MS500**** |
| Moving type | Track |
| Dimension (LxWxH) | 1910mm\*1150mm\*1345mm |
| Speed | 5km/h |
| Rated loading capacity | 520kg |
| Max. Reach | 1800mm |
| Pushing power | 8.2KN |
| Weight (without attachment) | 1050kgs |
| Hydraulic oil flow | 30L/min |
| Track oil flow | 46L/min |
| Oil tank capacity | 38L |
| Oil mode | L-HL46 |
| Battery capacity | 45Ah |
| Voltage | 12v |
| Ground Clearance | 150mm |